DATATYPE = CDS STUDY DEFINITION
FILENAME = cdscd_2.def
INSTRUME = CDS
DATE_CRE = 2001/08/24 12:59:54
END

LINELIST
    LL_ID    = 379
    DETECTOR = G
    LL_DESC  = GIS rebinned (x4)
    N_LINES  = 4
    LL_IND   = 1
        LINENAME = G2
        WAVELNTH = 267.105
        GR_ORDER = 1
        CEN_PIX  = 256
        WAVEBAND = 2
    LL_IND   = 2
        LINENAME = G1
        WAVELNTH = 159.729
        GR_ORDER = 1
        CEN_PIX  = 256
        WAVEBAND = 1
    LL_IND   = 3
        LINENAME = G3
        WAVELNTH = 404.731
        GR_ORDER = 1
        CEN_PIX  = 256
        WAVEBAND = 3
    LL_IND   = 4
        LINENAME = G4
        WAVELNTH = 673.458
        GR_ORDER = 1
        CEN_PIX  = 256
        WAVEBAND = 4

DATAWIN
    DW_ID    = 524
    DETECTOR = G
    DW_DESC  = 4 lines. {0}  dex = (512,1) pixels <56324>
    W_WIDTH  = 512
    W_HEIGHT = 1
    VDS_BACK = 0
    LL_ID    = 379
    N_WINS   = 4
    DW_IND   = 1
        WIN_NAME = WW_267_1                                
        WIN_DEF  = (3584,0,512,1)
        WIN_FLAG = 0
    DW_IND   = 2
        WIN_NAME = WW_159_7                                
        WIN_DEF  = (1536,0,512,1)
        WIN_FLAG = 0
    DW_IND   = 3
        WIN_NAME = WW_404_7                                
        WIN_DEF  = (5632,0,512,1)
        WIN_FLAG = 0
    DW_IND   = 4
        WIN_NAME = WW_673_5                                
        WIN_DEF  = (7680,0,512,1)
        WIN_FLAG = 0

RASTER
    RAS_ID   = 204
    DETECTOR = G
    RAS_DESC = Slit(4x240),Posns(30,1)@(4,0) steps
    SLIT_NUM = 5
    XSTEP    = 4
    YSTEP    = 0
    NX       = 30
    NY       = 1

RASTER_VAR
    RAS_ID   = 204
    RAS_VAR  = 1
    RV_DESC  = (120x240) arcsec, 3s <QUIET>  Comp. 1 IDs-(379,524)
    EXPTIME  = 3
    LL_ID    = 379
    COMP_ID  = 1
    COMP_OPT = 0
    DW_ID    = 524
    IEF_ID   = 0
    VDS_ORIENT = 0
    VDS_MAP  = 0
    TEL_RATE = M
    DURATION = 145
    USABLE   = Y

LINELIST
    LL_ID    = 380
    DETECTOR = N
    LL_DESC  = Corrected - Active region loop dynamics
    N_LINES  = 4
    LL_IND   = 1
        LINENAME = He I
        WAVELNTH = 584.33
        GR_ORDER = 1
        CEN_PIX  = 623
        WAVEBAND = 2
    LL_IND   = 2
        LINENAME = Fe XVI
        WAVELNTH = 360.761
        GR_ORDER = 1
        CEN_PIX  = 764
        WAVEBAND = 1
    LL_IND   = 3
        LINENAME = Mg IX
        WAVELNTH = 368.07
        GR_ORDER = 1
        CEN_PIX  = 868
        WAVEBAND = 1
    LL_IND   = 4
        LINENAME = O V
        WAVELNTH = 629.732
        GR_ORDER = 1
        CEN_PIX  = 1010
        WAVEBAND = 2

DATAWIN
    DW_ID    = 525
    DETECTOR = N
    DW_DESC  = Background,   4 lines. {0}  dex = (15,120) pixels <15209>
    W_WIDTH  = 15
    W_HEIGHT = 120
    VDS_BACK = 1
    LL_ID    = 380
    N_WINS   = 8
    DW_IND   = 1
        WIN_NAME = He_1_584_33                             
        WIN_DEF  = (616,392,15,120)
        WIN_FLAG = 0
    DW_IND   = 2
        WIN_NAME = Fe_16_360_76                            
        WIN_DEF  = (757,512,15,120)
        WIN_FLAG = 0
    DW_IND   = 3
        WIN_NAME = Mg_9_368_07                             
        WIN_DEF  = (861,512,15,120)
        WIN_FLAG = 0
    DW_IND   = 4
        WIN_NAME = O_5_629_73                              
        WIN_DEF  = (1003,392,15,120)
        WIN_FLAG = 0
    DW_IND   = 5
        WIN_NAME = Background                              
        WIN_DEF  = (20,20,10,10)
        WIN_FLAG = 0
    DW_IND   = 6
        WIN_NAME = Background                              
        WIN_DEF  = (994,20,10,10)
        WIN_FLAG = 0
    DW_IND   = 7
        WIN_NAME = Background                              
        WIN_DEF  = (20,994,10,10)
        WIN_FLAG = 0
    DW_IND   = 8
        WIN_NAME = Background                              
        WIN_DEF  = (994,994,10,10)
        WIN_FLAG = 0

RASTER
    RAS_ID   = 38
    DETECTOR = N
    RAS_DESC = Slit(4x240),Posns(30,-)@(4,-) steps
    SLIT_NUM = 5
    XSTEP    = 4
    YSTEP    = 0
    NX       = 30
    NY       = 1

RASTER_VAR
    RAS_ID   = 38
    RAS_VAR  = 46
    RV_DESC  = (120x240) arcsec, 5s <ACTIVE>  Comp. 2 IDs-(380,525)
    EXPTIME  = 5
    LL_ID    = 380
    COMP_ID  = 2
    COMP_OPT = 0
    DW_ID    = 525
    IEF_ID   = 0
    VDS_ORIENT = 0
    VDS_MAP  = 2
    TEL_RATE = M
    DURATION = 321
    USABLE   = Y

STUDY
    STUDY_ID = 258
    TITLE_ID = 525
    OBS_PROG = CDSCD
    TITLE    = CDS CORONAL DYNAMICS
    CATEGORY = S
    VAR_POINT = Y
    N_RASTER_DEF = 2
    RAS_IND   = 1
        RAS_ID   = 204
        POINTING = 1
        INS_X    = 0
        INS_Y    = 0
    RAS_IND   = 2
        RAS_ID   = 38
        POINTING = 1
        INS_X    = 0
        INS_Y    = 0

STUDY_VAR
    STUDY_ID = 258
    TITLE_ID = 525
    STUDYVAR = 2
    SV_DESC  = NIS AND GIS REBINNED (X4) VERSION 2
    N_RASTERS0 = 1
    DURATION0 = 145
    DURATION1 = 321
    ZONE_ID  = 5
    USABLE   = Y
    N_RASTER_DEF = 2
    RAS_IND   = 1
        RAS_ID   = 204
        RAS_VAR  = 1
        N_REPEAT_R = 1
    RAS_IND   = 2
        RAS_ID   = 38
        RAS_VAR  = 46
        N_REPEAT_R = 1
