DATATYPE = CDS STUDY DEFINITION
FILENAME = point_ew_1.def
INSTRUME = CDS
DATE_CRE = 2000/09/07 15:17:22
END

DATAWIN
    DW_ID    = 1
    DETECTOR = G
    DW_DESC  = GIS Band1234  <20484>
    W_WIDTH  = 2048
    W_HEIGHT = 1
    VDS_BACK = 0
    LL_ID    = 0
    N_WINS   = 4
    DW_IND   = 1
        WIN_NAME = BB_GIS_1                                
        WIN_DEF  = (0,0,2048,1)
        WIN_FLAG = 0
    DW_IND   = 2
        WIN_NAME = BB_GIS_2                                
        WIN_DEF  = (2048,0,2048,1)
        WIN_FLAG = 0
    DW_IND   = 3
        WIN_NAME = BB_GIS_3                                
        WIN_DEF  = (4096,0,2048,1)
        WIN_FLAG = 0
    DW_IND   = 4
        WIN_NAME = BB_GIS_4                                
        WIN_DEF  = (6144,0,2048,1)
        WIN_FLAG = 0

RASTER
    RAS_ID   = 72
    DETECTOR = G
    RAS_DESC = Slit(4x4),Posns(20,1)@(4,0) steps
    SLIT_NUM = 2
    XSTEP    = 4
    YSTEP    = 0
    NX       = 20
    NY       = 1

RASTER_VAR
    RAS_ID   = 72
    RAS_VAR  = 3
    RV_DESC  = (80x4) arcsec, 30s <QUIET>  Comp. 1 IDs-(0,1)
    EXPTIME  = 30
    LL_ID    = 0
    COMP_ID  = 1
    COMP_OPT = 0
    DW_ID    = 1
    IEF_ID   = 0
    VDS_ORIENT = 0
    VDS_MAP  = 0
    TEL_RATE = M
    DURATION = 637
    USABLE   = Y

LINELIST
    LL_ID    = 2
    DETECTOR = N
    LL_DESC  = VDS MOVIE SELECTION
    N_LINES  = 3
    LL_IND   = 1
        LINENAME = He I 584
        WAVELNTH = 584.33
        GR_ORDER = 1
        CEN_PIX  = 608
        WAVEBAND = 2
    LL_IND   = 2
        LINENAME = Mg IX 368
        WAVELNTH = 368.06
        GR_ORDER = 1
        CEN_PIX  = 864
        WAVEBAND = 1
    LL_IND   = 3
        LINENAME = O V 629
        WAVELNTH = 629.741
        GR_ORDER = 1
        CEN_PIX  = 996
        WAVEBAND = 2

DATAWIN
    DW_ID    = 4
    DETECTOR = N
    DW_DESC  = Background,   3 lines.  dex = (70,120) pixels <8357>
    W_WIDTH  = 70
    W_HEIGHT = 120
    VDS_BACK = 1
    LL_ID    = 2
    N_WINS   = 7
    DW_IND   = 1
        WIN_NAME = He_1_584_33                             
        WIN_DEF  = (573,392,70,120)
        WIN_FLAG = 0
    DW_IND   = 2
        WIN_NAME = Mg_9_368_06                             
        WIN_DEF  = (829,512,70,120)
        WIN_FLAG = 0
    DW_IND   = 3
        WIN_NAME = O_5_629_74                              
        WIN_DEF  = (961,392,62,120)
        WIN_FLAG = 0
    DW_IND   = 4
        WIN_NAME = Background                              
        WIN_DEF  = (20,20,10,10)
        WIN_FLAG = 0
    DW_IND   = 5
        WIN_NAME = Background                              
        WIN_DEF  = (994,20,10,10)
        WIN_FLAG = 0
    DW_IND   = 6
        WIN_NAME = Background                              
        WIN_DEF  = (20,994,10,10)
        WIN_FLAG = 0
    DW_IND   = 7
        WIN_NAME = Background                              
        WIN_DEF  = (994,994,10,10)
        WIN_FLAG = 0

RASTER
    RAS_ID   = 3
    DETECTOR = N
    RAS_DESC = Slit(90x240),Posns(1,-)@(0,-) steps
    SLIT_NUM = 6
    XSTEP    = 0
    YSTEP    = 0
    NX       = 1
    NY       = 1

RASTER_VAR
    RAS_ID   = 3
    RAS_VAR  = 3
    RV_DESC  = (90x240) arcsec, 10s <QUIET>  Comp. 1 IDs-(2,4)
    EXPTIME  = 10
    LL_ID    = 2
    COMP_ID  = 1
    COMP_OPT = 0
    DW_ID    = 4
    IEF_ID   = 0
    VDS_ORIENT = 0
    VDS_MAP  = 2
    TEL_RATE = M
    DURATION = 54
    USABLE   = Y

LINELIST
    LL_ID    = 254
    DETECTOR = N
    LL_DESC  = Reduced Synoptic line list + MgX
    N_LINES  = 5
    LL_IND   = 1
        LINENAME = HE  1  584.3
        WAVELNTH = 584.33
        GR_ORDER = 1
        CEN_PIX  = 611
        WAVEBAND = 2
    LL_IND   = 2
        LINENAME = Fe XVI
        WAVELNTH = 360.76
        GR_ORDER = 1
        CEN_PIX  = 758
        WAVEBAND = 1
    LL_IND   = 3
        LINENAME = MG  9  368.1
        WAVELNTH = 368.06
        GR_ORDER = 1
        CEN_PIX  = 862
        WAVEBAND = 1
    LL_IND   = 4
        LINENAME = Mg X
        WAVELNTH = 624.941
        GR_ORDER = 1
        CEN_PIX  = 957
        WAVEBAND = 2
    LL_IND   = 5
        LINENAME = O V 629.73
        WAVELNTH = 629.73
        GR_ORDER = 1
        CEN_PIX  = 998
        WAVEBAND = 2

DATAWIN
    DW_ID    = 495
    DETECTOR = N
    DW_DESC  = Background,   5 lines. {254}  dex = (24,120) pixels <20557>
    W_WIDTH  = 24
    W_HEIGHT = 120
    VDS_BACK = 1
    LL_ID    = 254
    N_WINS   = 9
    DW_IND   = 1
        WIN_NAME = He_1_584_33                             
        WIN_DEF  = (611,392,24,120)
        WIN_FLAG = 0
    DW_IND   = 2
        WIN_NAME = Fe_16_360_76                            
        WIN_DEF  = (752,512,24,120)
        WIN_FLAG = 0
    DW_IND   = 3
        WIN_NAME = Mg_9_368_06                             
        WIN_DEF  = (856,512,24,120)
        WIN_FLAG = 0
    DW_IND   = 4
        WIN_NAME = Mg_10_624_94                            
        WIN_DEF  = (957,392,24,120)
        WIN_FLAG = 0
    DW_IND   = 5
        WIN_NAME = O_5_629_73                              
        WIN_DEF  = (998,392,24,120)
        WIN_FLAG = 0
    DW_IND   = 6
        WIN_NAME = Background                              
        WIN_DEF  = (20,20,10,10)
        WIN_FLAG = 0
    DW_IND   = 7
        WIN_NAME = Background                              
        WIN_DEF  = (994,20,10,10)
        WIN_FLAG = 0
    DW_IND   = 8
        WIN_NAME = Background                              
        WIN_DEF  = (20,994,10,10)
        WIN_FLAG = 0
    DW_IND   = 9
        WIN_NAME = Background                              
        WIN_DEF  = (994,994,10,10)
        WIN_FLAG = 0

RASTER
    RAS_ID   = 31
    DETECTOR = N
    RAS_DESC = Slit(4x240),Posns(5,-)@(4,-) steps
    SLIT_NUM = 5
    XSTEP    = 4
    YSTEP    = 0
    NX       = 5
    NY       = 1

RASTER_VAR
    RAS_ID   = 31
    RAS_VAR  = 6
    RV_DESC  = (20x240) arcsec, 15s <QUIET>  Comp. 2 IDs-(254,495)
    EXPTIME  = 15
    LL_ID    = 254
    COMP_ID  = 2
    COMP_OPT = 0
    DW_ID    = 495
    IEF_ID   = 0
    VDS_ORIENT = 0
    VDS_MAP  = 2
    TEL_RATE = M
    DURATION = 101
    USABLE   = Y

STUDY
    STUDY_ID = 243
    TITLE_ID = 493
    OBS_PROG = POINT_EW
    TITLE    = E/W POINTING TEST
    CATEGORY = C
    VAR_POINT = Y
    N_RASTER_DEF = 3
    RAS_IND   = 1
        RAS_ID   = 72
        POINTING = 1
        INS_X    = 0
        INS_Y    = 0
    RAS_IND   = 2
        RAS_ID   = 3
        POINTING = 1
        INS_X    = 0
        INS_Y    = 0
    RAS_IND   = 3
        RAS_ID   = 31
        POINTING = 1
        INS_X    = 0
        INS_Y    = 0

STUDY_VAR
    STUDY_ID = 243
    TITLE_ID = 493
    STUDYVAR = 1
    SV_DESC  = VAR 1
    N_RASTERS0 = 2
    DURATION0 = 691
    DURATION1 = 101
    ZONE_ID  = 4
    USABLE   = Y
    N_RASTER_DEF = 3
    RAS_IND   = 1
        RAS_ID   = 72
        RAS_VAR  = 3
        N_REPEAT_R = 1
    RAS_IND   = 2
        RAS_ID   = 3
        RAS_VAR  = 3
        N_REPEAT_R = 1
    RAS_IND   = 3
        RAS_ID   = 31
        RAS_VAR  = 6
        N_REPEAT_R = 1
