DATATYPE = CDS STUDY DEFINITION
FILENAME = cloops2_2.def
INSTRUME = CDS
DATE_CRE = 1996/08/05 10:02:00
END

LINELIST
    LL_ID    = 97
    DETECTOR = N
    LL_DESC  = Loop List
    N_LINES  = 7
    LL_IND   = 1
        LINENAME = O IV
        WAVELNTH = 554.52
        GR_ORDER = 1
        CEN_PIX  = 356
        WAVEBAND = 2
    LL_IND   = 2
        LINENAME = Fe XIV
        WAVELNTH = 334.17
        GR_ORDER = 1
        CEN_PIX  = 380
        WAVEBAND = 1
    LL_IND   = 3
        LINENAME = Fe XII
        WAVELNTH = 338.26
        GR_ORDER = 1
        CEN_PIX  = 438
        WAVEBAND = 1
    LL_IND   = 4
        LINENAME = He I
        WAVELNTH = 584.33
        GR_ORDER = 1
        CEN_PIX  = 610
        WAVEBAND = 2
    LL_IND   = 5
        LINENAME = Fe XVI
        WAVELNTH = 360.76
        GR_ORDER = 1
        CEN_PIX  = 759
        WAVEBAND = 1
    LL_IND   = 6
        LINENAME = Fe XII
        WAVELNTH = 364.47
        GR_ORDER = 1
        CEN_PIX  = 811
        WAVEBAND = 1
    LL_IND   = 7
        LINENAME = Mg IX
        WAVELNTH = 368.06
        GR_ORDER = 1
        CEN_PIX  = 863
        WAVEBAND = 1

DATAWIN
    DW_ID    = 129
    DETECTOR = N
    DW_DESC  = Background,   7 lines.  dex = (21,120) pixels <12614>
    W_WIDTH  = 21
    W_HEIGHT = 120
    VDS_BACK = 1
    LL_ID    = 97
    N_WINS   = 11
    DW_IND   = 1
        WIN_NAME = O_4_554_52                              
        WIN_DEF  = (346,392,21,120)
        WIN_FLAG = 0
    DW_IND   = 2
        WIN_NAME = Fe_14_334_17                            
        WIN_DEF  = (370,512,21,120)
        WIN_FLAG = 0
    DW_IND   = 3
        WIN_NAME = Fe_12_338_26                            
        WIN_DEF  = (428,512,21,120)
        WIN_FLAG = 0
    DW_IND   = 4
        WIN_NAME = He_1_584_33                             
        WIN_DEF  = (600,392,21,120)
        WIN_FLAG = 0
    DW_IND   = 5
        WIN_NAME = Fe_16_360_76                            
        WIN_DEF  = (749,512,21,120)
        WIN_FLAG = 0
    DW_IND   = 6
        WIN_NAME = Fe_12_364_47                            
        WIN_DEF  = (801,512,21,120)
        WIN_FLAG = 0
    DW_IND   = 7
        WIN_NAME = Mg_9_368_06                             
        WIN_DEF  = (853,512,21,120)
        WIN_FLAG = 0
    DW_IND   = 8
        WIN_NAME = Background                              
        WIN_DEF  = (20,20,10,10)
        WIN_FLAG = 0
    DW_IND   = 9
        WIN_NAME = Background                              
        WIN_DEF  = (994,20,10,10)
        WIN_FLAG = 0
    DW_IND   = 10
        WIN_NAME = Background                              
        WIN_DEF  = (20,994,10,10)
        WIN_FLAG = 0
    DW_IND   = 11
        WIN_NAME = Background                              
        WIN_DEF  = (994,994,10,10)
        WIN_FLAG = 0

RASTER
    RAS_ID   = 56
    DETECTOR = N
    RAS_DESC = Area(80x240),slit(4x240),Posns(20,-)@(4,-) steps
    SLIT_NUM = 5
    XSTEP    = 4
    YSTEP    = 0
    NX       = 20
    NY       = 1

RASTER_VAR
    RAS_ID   = 56
    RAS_VAR  = 2
    RV_DESC  = (80x240) arcsec, 6s <QUIET>  Comp. 2 IDs-(97,129)
    EXPTIME  = 6
    LL_ID    = 97
    COMP_ID  = 2
    COMP_OPT = 0
    DW_ID    = 129
    IEF_ID   = 0
    VDS_ORIENT = 0
    VDS_MAP  = 2
    TEL_RATE = M
    DURATION = 480
    USABLE   = Y

STUDY
    STUDY_ID = 78
    TITLE_ID = 216
    OBS_PROG = CLOOPS2
    TITLE    = CORONAL LOOPS STUDY - NI PART
    CATEGORY = S
    VAR_POINT = Y
    N_RASTER_DEF = 1
    RAS_IND   = 1
        RAS_ID   = 56
        POINTING = 1
        INS_X    = 0
        INS_Y    = 0

STUDY_VAR
    STUDY_ID = 78
    TITLE_ID = 216
    STUDYVAR = 2
    SV_DESC  = FIRST ATTEMPT
    N_RASTERS0 = 0
    DURATION0 = 0
    DURATION1 = 480
    ZONE_ID  = 4
    USABLE   = Y
    N_RASTER_DEF = 1
    RAS_IND   = 1
        RAS_ID   = 56
        RAS_VAR  = 2
        N_REPEAT_R = 1
