DATATYPE = CDS STUDY DEFINITION
FILENAME = cosar_1_43.def
INSTRUME = CDS
DATE_CRE = 1998/02/26 09:29:08
END

LINELIST
    LL_ID    = 172
    DETECTOR = N
    LL_DESC  = COSAR No.4
    N_LINES  = 6
    LL_IND   = 1
        LINENAME = Fe XIV
        WAVELNTH = 334.17
        GR_ORDER = 1
        CEN_PIX  = 380
        WAVEBAND = 1
    LL_IND   = 2
        LINENAME = He I
        WAVELNTH = 584.33
        GR_ORDER = 1
        CEN_PIX  = 610
        WAVEBAND = 2
    LL_IND   = 3
        LINENAME = Fe XIV
        WAVELNTH = 353.83
        GR_ORDER = 1
        CEN_PIX  = 660
        WAVEBAND = 1
    LL_IND   = 4
        LINENAME = Fe XVI
        WAVELNTH = 360.761
        GR_ORDER = 1
        CEN_PIX  = 758
        WAVEBAND = 1
    LL_IND   = 5
        LINENAME = Mg IX
        WAVELNTH = 368.06
        GR_ORDER = 1
        CEN_PIX  = 863
        WAVEBAND = 1
    LL_IND   = 6
        LINENAME = O V
        WAVELNTH = 629.73
        GR_ORDER = 1
        CEN_PIX  = 998
        WAVEBAND = 2

DATAWIN
    DW_ID    = 317
    DETECTOR = N
    DW_DESC  = Background,   6 lines. {172}  dex = (31,120) pixels <12053>
    W_WIDTH  = 31
    W_HEIGHT = 120
    VDS_BACK = 1
    LL_ID    = 172
    N_WINS   = 10
    DW_IND   = 1
        WIN_NAME = Fe_14_334_17                            
        WIN_DEF  = (365,512,31,120)
        WIN_FLAG = 0
    DW_IND   = 2
        WIN_NAME = He_1_584_33                             
        WIN_DEF  = (596,392,31,120)
        WIN_FLAG = 0
    DW_IND   = 3
        WIN_NAME = Fe_14_353_83                            
        WIN_DEF  = (645,512,31,120)
        WIN_FLAG = 0
    DW_IND   = 4
        WIN_NAME = Fe_16_360_76                            
        WIN_DEF  = (743,512,31,120)
        WIN_FLAG = 0
    DW_IND   = 5
        WIN_NAME = Mg_9_368_06                             
        WIN_DEF  = (847,512,31,120)
        WIN_FLAG = 0
    DW_IND   = 6
        WIN_NAME = O_5_629_73                              
        WIN_DEF  = (983,392,31,120)
        WIN_FLAG = 0
    DW_IND   = 7
        WIN_NAME = Background                              
        WIN_DEF  = (20,20,10,10)
        WIN_FLAG = 0
    DW_IND   = 8
        WIN_NAME = Background                              
        WIN_DEF  = (994,20,10,10)
        WIN_FLAG = 0
    DW_IND   = 9
        WIN_NAME = Background                              
        WIN_DEF  = (20,994,10,10)
        WIN_FLAG = 0
    DW_IND   = 10
        WIN_NAME = Background                              
        WIN_DEF  = (994,994,10,10)
        WIN_FLAG = 0

RASTER
    RAS_ID   = 36
    DETECTOR = N
    RAS_DESC = Slit(2x240),Posns(60,-)@(2,-) steps
    SLIT_NUM = 4
    XSTEP    = 2
    YSTEP    = 0
    NX       = 60
    NY       = 1

RASTER_VAR
    RAS_ID   = 36
    RAS_VAR  = 46
    RV_DESC  = (120x240) arcsec, 10s <QUIET>  Comp. 2 IDs-(172,317)
    EXPTIME  = 10
    LL_ID    = 172
    COMP_ID  = 2
    COMP_OPT = 0
    DW_ID    = 317
    IEF_ID   = 0
    VDS_ORIENT = 0
    VDS_MAP  = 2
    TEL_RATE = H
    DURATION = 1011
    USABLE   = Y

STUDY
    STUDY_ID = 41
    TITLE_ID = 122
    OBS_PROG = COSAR_1
    TITLE    = CORONAL STRUCTURE ABOVE ACTIVE REGION - II
    CATEGORY = S
    VAR_POINT = Y
    N_RASTER_DEF = 1
    RAS_IND   = 1
        RAS_ID   = 36
        POINTING = 1
        INS_X    = 0
        INS_Y    = 0

STUDY_VAR
    STUDY_ID = 41
    TITLE_ID = 122
    STUDYVAR = 43
    SV_DESC  = 10 S, 6 LINES, HI-RATE
    N_RASTERS0 = 0
    DURATION0 = 0
    DURATION1 = 1011
    ZONE_ID  = 4
    USABLE   = Y
    N_RASTER_DEF = 1
    RAS_IND   = 1
        RAS_ID   = 36
        RAS_VAR  = 46
        N_REPEAT_R = 1
