DATATYPE = CDS STUDY DEFINITION
FILENAME = /mn/schedar/u1/nilsbr/o_loop4_2.def
INSTRUME = CDS
DATE_CRE = 2000/08/31 09:16:37
END

LINELIST
    LL_ID    = 219
    DETECTOR = N
    LL_DESC  = Loop Dynamics 1a List
    N_LINES  = 6
    LL_IND   = 1
        LINENAME = New VDS line
        WAVELNTH = 562.769
        GR_ORDER = 1
        CEN_PIX  = 426
        WAVEBAND = 2
    LL_IND   = 2
        LINENAME = He I 584
        WAVELNTH = 584.33
        GR_ORDER = 1
        CEN_PIX  = 610
        WAVEBAND = 2
    LL_IND   = 3
        LINENAME = New VDS line
        WAVELNTH = 599.661
        GR_ORDER = 1
        CEN_PIX  = 741
        WAVEBAND = 2
    LL_IND   = 4
        LINENAME = Fe XVI 360
        WAVELNTH = 360.76
        GR_ORDER = 1
        CEN_PIX  = 758
        WAVEBAND = 1
    LL_IND   = 5
        LINENAME = Mg IX 368
        WAVELNTH = 368.06
        GR_ORDER = 1
        CEN_PIX  = 862
        WAVEBAND = 1
    LL_IND   = 6
        LINENAME = O V 629
        WAVELNTH = 629.73
        GR_ORDER = 1
        CEN_PIX  = 997
        WAVEBAND = 2

DATAWIN
    DW_ID    = 293
    DETECTOR = N
    DW_DESC  = Background, 6 lines. {0}  dex = (15,120) pixels <11890>
    W_WIDTH  = 15
    W_HEIGHT = 120
    VDS_BACK = 1
    LL_ID    = 219
    N_WINS   = 10
    DW_IND   = 1
        WIN_NAME = WW_562_77
        WIN_DEF  = (419,392,15,120)
        WIN_FLAG = 0
    DW_IND   = 2
        WIN_NAME = He_1_584_33
        WIN_DEF  = (603,392,15,120)
        WIN_FLAG = 0
    DW_IND   = 3
        WIN_NAME = WW_599_66
        WIN_DEF  = (734,392,15,120)
        WIN_FLAG = 0
    DW_IND   = 4
        WIN_NAME = Fe_16_360_76
        WIN_DEF  = (751,512,15,120)
        WIN_FLAG = 0
    DW_IND   = 5
        WIN_NAME = Mg_9_368_06
        WIN_DEF  = (855,512,15,120)
        WIN_FLAG = 0
    DW_IND   = 6
        WIN_NAME = O_5_629_73
        WIN_DEF  = (990,392,15,120)
        WIN_FLAG = 0
    DW_IND   = 7
        WIN_NAME = Background
        WIN_DEF  = (20,20,10,10)
        WIN_FLAG = 0
    DW_IND   = 8
        WIN_NAME = Background
        WIN_DEF  = (994,20,10,10)
        WIN_FLAG = 0
    DW_IND   = 9
        WIN_NAME = Background
        WIN_DEF  = (20,994,10,10)
        WIN_FLAG = 0
    DW_IND   = 10
        WIN_NAME = Background
        WIN_DEF  = (994,994,10,10)
        WIN_FLAG = 0

RASTER
    RAS_ID   = 102
    DETECTOR = N
    RAS_DESC = Slit(4x240),Posns(40,-)@(0,-) steps
    SLIT_NUM = 5
    XSTEP    = 0
    YSTEP    = 0
    NX       = 40
    NY       = 1

RASTER_VAR
    RAS_ID   = 102
    RAS_VAR  = 2
    RV_DESC  = (4x240) arcsec, 10s <QUIET>  Comp. 2 IDs-(219,293)
    EXPTIME  = 10
    LL_ID    = 219
    COMP_ID  = 2
    COMP_OPT = 0
    DW_ID    = 293
    IEF_ID   = 0
    VDS_ORIENT = 0
    VDS_MAP  = 2
    TEL_RATE = M
    DURATION = 615
    USABLE   = Y

STUDY
    STUDY_ID = 125
    TITLE_ID = 355
    OBS_PROG = O_LOOP4
    TITLE    = LOOP DYNAMICS STUDY 4
    CATEGORY = S
    VAR_POINT = Y
    N_RASTER_DEF = 1
    RAS_IND   = 1
        RAS_ID   = 102
        POINTING = 1
        INS_X    = 0
        INS_Y    = 0

STUDY_VAR
    STUDY_ID = 125
    TITLE_ID = 355
    STUDYVAR = 2
    SV_DESC  = VAR. 2, 4x240 ARCSEC
    N_RASTERS0 = 0
    DURATION0 = 0
    DURATION1 = 615
    ZONE_ID  = 1
    USABLE   = Y
    N_RASTER_DEF = 1
    RAS_IND   = 1
        RAS_ID   = 102
        RAS_VAR  = 2
        N_REPEAT_R = 1
